Dahua Pro PTZ Camera Driver
Help: https://help.drivercentral.io
Installation Note: It is recommended to connect directly to cameras.  IP camera video streams that must be reprocessed through the NVR have slower link up times to Control4.
Setup Direct Camera Method (preferred method)

•	Select Driver Action: Set Driver for Direct Camera Access
•	Enter credentials for camera access

Setup NVR/XVR Connection Method

•	Bind Driver to NVR Channel (requires nvr driver: Dahua Pro NVR Driver)
•	Refresh Navigators/Test

Video Stream Selection:  Cameras transmit video via a video stream.  Each NVR or Camera will have settings to adjust main stream or sub stream(s).

Video Stream Settings: Configuration of the video streams is recommended.  Below are the typical settings an installer should set the video to:
	Code-Stream Type: Continuous
	Compression: H.264
	Resolution: 1280*720(720P)
	Frame Rate(FPS): 10
	Bit Rate Type: CBR
	Bit Rate: 1024

Testing Camera Video: Click on Camera Test and Run Snapshot and H.264.  MJPEG is only required if HC250, HC800 or T2 Touchscreens are installed in job.  Note: if MJPEG is required, MJPEG video stream must be configured on NVR/Camera

About Driver Notes:
	This driver contains code written by Cinegration LLC.  Any modification to this driver without the express written permission or without the express consent by Cinegration will void all warranties, constitute a ban on all drivers released by Cinegration and potentially legal action.
	This driver has been designed to work with Control4 2.9.1 and higher Control4 systems.

Developed by: Cinegration LLC.  www.cinegration.com/drivers