Driver for Integration NovaStar 
LED Panel Controllers
Series V760 – V960 and similar

Objective:
Integration to the Control4 solution

Requirements:
Control4 system running version 2.10 or higher

Propriedades do driver:
Debug Mode
On | Off
Used for activity tracking, typically by the developer
Power On Delay-Milliseconds
Time in milliseconds that it takes the dashboard to turn on. Default 4000 (4 seconds)
Command Delay-Milliseconds
Interval in ms between commands
IP
Enter NovaStar IP. Reserve this IP on DHCP router table or leave fixed on Novastar device
TCP Port
Communication port, standard 5201
IP Conn Status
IP connection information from the driver to the device
Connection
Connection type. IP or Serial
Send HEXA
Field for sending codes for tests

Actions - Programming
Send Command (without checksum)
Send all frame 

Send Complete Command
Send frame without chcksum. Driver will calculate 

Mode
Normal | Freeze | Black

Presets
Load, Save or Delete, Presets from 0 to 255 (or maximum supported by device)

Send Brightness
Brightness value between 0 to 255

Change Log 
Version 1060	21/dec/2025	Initial Version