Dahua Pro NVR Driver
Support: https://help.drivercentral.io
Driver Overview:  Enables the use of the Monitor-Out/HDMI/VGA connector to integrate into Customers Control4 (creates Watch NVR Icon on Control4 systems).  This driver also supports ‘linking’ to the camera interface in Control4 via the Cinegration Fixed/PTZ Cameras.

Setup
•	Enter IP under Network Connections

•	Enter credentials for NVR.  Note: If incorrect password is entered, reboot NVR and try again.
•	Set # of Channels and configure any options for NVR
•	Make bindings to AV equipment
•	Refresh Navigators
•	Below is a picture of a successful connection to NVR.

Event Notification from NVR
The NVR has many triggers. These can be used for custom Control4 programming via the Events tab or creating a sensor connection and use the connection bindings.  The last event information is also stored in Composer Variables for dealer customization of the smart home.  
Use Contact Sensors to do triggering:

Or via Event Programming:

About Driver Notes:
	This driver contains code written by Cinegration LLC.  Any modification to this driver without the express written permission or without the express consent by Cinegration will void all warranties, constitute a ban on all drivers released by Cinegration and potentially legal action.
	This driver has been designed to work with Control4 2.10.0 and higher Control4 systems.