Integration via Netatmo
Require Hardware:
MyHomeServer1
or
Living Now Gateway 
Integration through these Gateway lines is done through the Netatmo Connect System - netatmo.com
To do this, you need to create an "Application" using the customer's data in the Home + Control application
This integration does not allow instant feedback when a load is accessed manually on keypad or Home + Control App. Feedback on Control4 can take until 30 seconds, it is done by polling, driver check device states and update loads when necessary
Creating the Netatmo Application
Access via web browser:
https://dev.netatmo.com/apps/createanapp#form

Fill in the form with customer data. Use your website address if one doesn't exist

On the next page, copy and save this data (Client ID and Clientsecret):

Generate a Token selecting all “Scopes”

On the next page, grant permission to the Application:

Save thise keys, Access Token and Refresh Token

Configuring the Driver 4Drivers:

Enter data into the main driver:

Request the “Home” list within the client's project. There will probably be only one:

Select properly Home:

Now see the documentation on the Lighting or Curtain drivers

Property Netatmo Cloud Status shows last Authorization process or fail in process
If driver lost authentication will necessary Reset Keys on App Page and fill all data on driver property

We are checking with Netatmo a best approach to Authentication on this driver 

In case of more than one “Home” on project, create an APP for each one.

Change Log
1051	19/Ago/2023	Initial Version
1052	10/Jun/2024	Fix on Lighting Type Commands
1053	15/Jun/2024	Changes on Validation Processs
1054	20/Jun/2024	Fix on ONOFF Lights commands
1055	20/Nov/2024	Change on driver License Validation